Minimum cost flow

a b=5